**Penalty shoot out Risk Assessment**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***Hazard*** | ***Existing Control Measures*** | ***Harm******(1-5)*** | ***Likely******(1-5)*** | ***Risk******(1-5)*** | ***Further Controls to Reduce Risk*** |
| Over enthusiastic participants | Responsible person supervising at all times | 1 | 1 | 1 | On site training given  |
| Jumping off unit | Responsible person supervising at all times.Safety mats around entry/exit to the  | 1 | 1 | 1 | In the event of large numbers participants are controlled on and off of the castle in timed groups. |
| Larger participants colliding with smaller participants | Responsible person supervising at all times | 1 | 1 | 1 | Participants put in to groups of similar size. |
| Tripping over anchorage points, spare equipment, electrical cables | Anchor points used as per manufacturers instructions and spare equipment erected safely or stowed away. Where possible electrical cable does not cross any public pathway.  | 1 | 1 | 1 | In the event of large numbers of participants attending or large events, additional safety fencing is erected, electrical cables will be erected overhead or covered and suitably marked.  |
| Petrol Blower, GeneratorRisk of fire | Safety fencing erected around blower/generator.Blowers/generators filled with fuel before delivery Suitable fire extinguisher supplied, units are fire retardant, electrical equipment is PAT tested  | 3 | 1 | 1 | All spare fuel is stored in suitable marked container, and in a safe location, units switched off during re fuelling, |

**The above information is based on manufacturer’s criteria and experience from extensive use of the equipment.**

|  |
| --- |
| Any notes, New risks: Venue to supply barrier fencing to keep the public at a safe distance,    |

|  |  |  |
| --- | --- | --- |
| Are all risks acceptable: (please circle) | Yes | No |
| Risk Assessment Carried out by |   | Signed |   | Date: |
| Checked By |   | Signed |   | Date: |